# NOTICE TO CONTRACTORS

Sealed Bids will be received by DOUGLAS COUNTY SCHOOL DISTRICT #10, ELKHORN PUBLIC SCHOOLS at the office of LAMP RYNEARSON, INC. (ENGINEER), 14710 WEST DODGE ROAD, SUITE 100, OMAHA, NEBRASKA, until 4:30 P.M., MAY 7, 2019, for furnishing all labor, tools, materials, and equipment required for the project designated as SANITARY SEWER, STORM SEWER, AND PAVING – IDA POINTE NORTH, and all other work necessary or incidental thereto, as per plans and specifications on file at the office of said Engineer, at which time Bids will be publicly opened, read aloud, and tabulated. The extent of the work involved and the materials to be bid upon are as follows:

| **ITEMNO.** | **BID ITEM DESCRIPTION** | **APPROXIMATE QUANTITY** |
| --- | --- | --- |
|  | **SANITARY** |
| 1 | CLEARING AND GRUBBING GENERAL | 1 | LS |
| 2 | DEWATERING | 10 | DY |
| 3 | CONSTRUCT 8" SANITARY SEWER PIPE | 2,100 | LF |
| 4 | CONSTRUCT 8" PIPE BEDDING | 2,100 | LF |
| 5 | CONSTRUCT 54" I.D. SANITARY MANHOLE (11 EA) | 145 | VF |
| 6 | CONSTRUCT MANHOLE RING COLLAR | 2 | EA |
| 7 | CONSTRUCT EXTERNAL FRAME SEAL | 1 | EA |
| 8 | CONSTRUCT 8" PIPE PLUG | 3 | EA |
| 9 | CONSTRUCT MANHOLE OVER EXISTING PIPE | 2 | EA |
| 10 | STABILIZATION TRENCH W/ CRUSHED LIMESTONE | 100 | TN |
| 11 | STABILIZATION TRENCH W/ TYPE "A" RIP RAP | 200 | TN |
| 12 | FURNISH AND INSTALL GEOTEXTILE FABRIC | 1,000 | SY |
| 13 | FURNISH AND INSTALL GEOGRID | 1,000 | SY |
|  | **STORM** |
| 1 | GENERAL GRADING AND SHAPING | 1 | LS |
| 2 | CONSTRUCT 18" R.C.P., CLASS III | 150 | LF |
| 3 | CONSTRUCT 24" R.C.P., CLASS III | 90 | LF |
| 4 | CONSTRUCT 30" R.C.P., CLASS III | 120 | LF |
| 5 | CONSTRUCT 36" R.C.P., CLASS III | 410 | LF |
| 6 | CONSTRUCT 54" TYPE II AREA INLET (1 EA) | 8 | VF |
| 7 | CONSTRUCT 18" R.C. FLARED END SECTION | 2 | EA |
| 8 | CONSTRUCT 30" R.C. FLARED END SECTION | 1 | EA |
| 9 | CONSTRUCT 36" R.C. FLARED END SECTION | 1 | EA |
| 10 | CONSTRUCT 18" PIPE BEDDING | 150 | LF |
| 11 | CONSTRUCT 24" PIPE BEDDING | 90 | LF |
| 12 | CONSTRUCT 30" PIPE BEDDING | 120 | LF |
| 13 | CONSTRUCT 36" PIPE BEDDING | 410 | LF |
| 14 | CONSTRUCT TEMPORARY INLET BASE | 3 | EA |
| 15 | STABILIZE TRENCH W/ CRUSHED LIMESTONE | 100 | TN |
| 16 | CONSTRUCT RIP RAP APRON "TYPE A" | 50 | TN |
| 17 | STABILIZATION TRENCH W/ TYPE "A" RIP RAP | 50 | TN |
| 18 | FURNISH AND INSTALL GEOTEXTILE FABRIC | 500 | SY |
| 19 | TEMPORARY SEEDING | 2 | AC |
| 20 | CONSTRUCT SILT FENCE | 1,000 | LF |
| 21 | CLEANOUT SILT FENCE | 1,000 | LF |
| 22 | REMOVE SILT FENCE | 1,000 | LF |
| 23 | CLEANOUT SILT BASIN | 6,000 | CY |
| 24 | RE-CONSTRUCT SEDIMENT TRAP | 2,000 | CY |
| 25 | CONSTRUCT ROCK ACCESS ROAD | 300 | TN |
|  | **PAVING** |
| 1 | 7" CONCRETE PAVEMENT - TYPE L65 | 6,950 | SY |
| 2 | 9" CONCRETE PAVEMENT - TYPE L65 | 1,850 | SY |
| 3 | COMMON EARTH EXCAVATION | 2,933 | CY |
| 4 | CONSTRUCT CURB INLET | 8 | EA |
| 5 | ADJUST MANHOLE TO GRADE (11 SAN) | 11 | EA |
| 6 | CONSTRUCT EXTERNAL FRAME SEAL (10 SAN) | 10 | EA |
| 7 | CONSTRUCT THICKENED EDGE | 50 | LF |
| 8 | CONSTRUCT TEMPORARY TURNAROUND | 1 | EA |
| 9 | CONSTRUCT END OF STREEET BARRICADE | 1 | EA |
| 10 | CONSTRUCT END OF STREET GABION STRUCTURE | 1 | EA |
| 11 | JET EXISTING SANITARY SEWER | 2,100 | LF |
| 12 | CONSTRUCT 7" PCC PAVEMENT WITH INTEGRAL 4" SPEED TABLE | 1 | EA |
| 13 | CONSTRUCT MEDIAN NOSE | 6 | EA |
| 14 | CONSTRUCT 6" MEDIAN SURFACING | 662 | SF |
| 15 | CONSTRUCT POST MOUNTED SIGN | 12 | EA |
| 16 | PERFORMED PAVEMENT MARKING - 5" YELLOW | 368 | LF |
| 17 | PERFORMED PAVEMENT MARKING - 8" WHITE | 36 | LF |
| 18 | PERFORMED PAVEMENT MARKING - 24" WHITE | 96 | LF |
| 19 | DETECTABLE WARNING PANEL | 48 | SF |
| 20 | REMOVE TEMP INLET BASE | 3 | EA |

Complete digital project bidding documents are available online for viewing or download purchase. Go to
[www.LampRynearson.com](http://www.LampRynearson.com) and select QUESTCDN at the bottom of page or contact [www.questcdn.com](http://www.questcdn.com) and use the Project Search page. Plan sets can be downloaded and saved for $20.00 at either site utilizing eBidDoc™#**6236703.** Contact QuestCDN at 952-233-1632 or info@questcdn.com for assistance if needed. An optional paper set of bidding documents may be obtained from the Engineer upon pre-payment by cash, check, or using prepaid account with Engineer of $50.00 if picked up and $60.00 if mailed (both non-refundable). Contractor must give 24-hour notice to Engineer when picking up paper sets*.*

All bids must be submitted on bid forms furnished by Lamp Rynearson, Inc. and must be enclosed in an envelope, sealed and addressed to DOUGLAS COUNTY SCHOOL DISTRICT #10, ELKHORN PUBLIC SCHOOLS and shall be marked “PROPOSAL FOR SANITARY SEWER, STORM SEWER AND PAVING – IDA POINTE NORTH” with the bidder’s name and address on said envelope. The Bid Security shall be in a separate sealed envelope attached to the Proposal envelope and shall be marked “BID SECURITY FOR SANITARY SEWER, STORM SEWER AND PAVING – IDA POINTE NORTH” with the bidder’s name and address on said envelope.

The Bid Security in the form of a certified check, a cashier’s check or Bid Bond (on EJCDC Form No. C-430), in the amount of FIVE (5%) PERCENT OF TOTAL BID AMOUNT of bid shall be payable without condition to DOUGLAS COUNTY SCHOOL DISTRICT #10, ELKHORN PUBLIC SCHOOLS as a guarantee the bidder, if successful, will execute the contract and provide an acceptable Contract Bond from an approved surety in the amount of 100 percent of the contract price.

No bidder may withdraw their Bid for a period of THIRTY (30) days after the date set for the opening of bids. The Owner reserves the right to reject any or all bids and to waive informalities.

Upon approval, the Owner will issue payment to the Contractor in the amount of 90% of the contracted value of the completed work as of the end of the preceding month, as recommended by the Engineer. Payment for the balance retained will be issued by the Owner upon completion of the work and approval thereof by the Owner's Engineer, City or Governmental approval when necessary, and acceptance by the Owner.

.